{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["附件一 2022年下半年电工电子类教学耗材需求明细表"],"read":"whole","date_system":"1900"}

{"sheet":"附件一 2022年下半年电工电子类教学耗材需求明细表","index":0,"n_rows":77,"n_cols":8,"rows_kept":77,"merged":[[0,0,0,7]]}
["附件：先进制造学院       2024年上半年自动化类教学耗材需求明细表"]
["编号","货物名称","规格型号","单位","数量","单价（元）","小计（元）","备注"]
[1,"气阀","DC 24V   4.8w","个",3,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[2,"小型推拉气缸","      MA16X25-S-CA  ","个",3,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[3,"光纤传感器","       FF系列","个",3,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[4,"光电传感器","     G18-3A30NA    24V","个",3,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[5,"接近开关","       F3N-18T ","个",3,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[6,"导轨式电源","FP300D-24MDA FP300D-48MDA","个",4,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[7," 小型直流电机","定做DC 24V","个",3,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[8,"螺丝批","合资 平头及十字头  6.5*150mm","套",6]
[9,"镀锡连接裸线","Φ0.6","斤",20]
[10,"焊锡丝","φ0.8mm  进口阿华(蓝标)\n1kg 粒装","粒",20]
[11,"数字万用表","胜利牌  vc890C+","个",10]
[12,"自动化实验套件（核心板）","成品套件\n实验套件能够完成各种基础资源的实验，能够完成外接温度传感器、、温湿度传感器、蓝牙实验、wifi实验，流水灯、数码管、lora通信实验，RS485通信、24c02存储器芯片读取，ds1302、红外等实验。","套",100,null,null,"与教材配套，有提供图纸"]
[13,"实验板连接、杜邦线",null,"套",100]
[14,"自动化外围套件","教学实验散件                  蜂鸣器模块、超声波模块、光敏模块等","套",100,null,null,"须与教材配套，有提供图纸"]
[15,"功放模块","150w*2","套",2]
[16,"10w LED","10w 900-1000lm  LED","套",10]
[17,"12V震动电机","12V 8500转/min 单头","个",4]
[18,"6V震动电机","6V 8500转/min  单头","个",4]
[19,"黑色亚克力板","60*60*0.5cm  磨砂 黑色","块",10]
[20,"透明亚克力板","40*40*0.5cm   透明","块",10]
[21,"芯片CH32V203F8P6","TSSOP-20","片",10]
[22,"芯片BQ76920","BQ7692003PWR TSSOP20","片",10]
[23,"自动化控制应用样板","接插板、接触器、道轨","套",2]
[24,"毫安表","定做","个",40]
[25,"电压表","6L2正泰或环宇,30v","个",20]
[26,"钮扣电池2032",null,"粒",10]
[27,"电源插头","进口","条",20]
[28,"元器件货架","定做","个",8,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[29,"变压器","3w   永星","个",20]
[30,"控制变压器","BK-100VA     电压定制","台",10]
[31,"JS-999接线柱","红色","粒",100,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[32,"JS-999接线柱","黑色","粒\n\n",100,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[33,"熔断器座","RT28N一32X 3P正泰或环宇电器","个",30,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[34,"保险管","R015   2A .3A  6A","粒",150]
[35,"小开关","8*8  三脚","只",100]
[36,"剥线钳","ST1041","支",3]
[37,"自动空气开关","NM1-63S/3300","个",10,null,null,"需到实验室现场更换或安装，并与实验室设备配套"]
[38,"内六角",null,"支",30]
[39,"触摸屏电阻全套",null,"套",1]
[40,"实验箱 插线","双头灯笼插头(连线约50cm)","袋",8,null,null,"每袋50条 与实验室设备配套，提供样品"]
[41,"万用表","上海星牌 500型  配电池","个",1]
[42,"万用表","上海星牌 368型  配电池","个",5]
[43,"工具箱","含20种工具","套",4]
[44,"精密螺丝刀",null,"套",2]
[45,"手机支架","2.1米","支",5]
[46,"压线钳","裸端子","支",3]
[47,"压线钳","绝缘端子","支",3]
[48,"数字型钳表","胜利vc606A","支",10]
[49,"12目接线端子","TB-2512 铜","支",60]
[50,"10目接线端子","TB-2510 铜","支",5]
[51,"黄金铝壳电阻","100w100欧","个",120]
[52,"螺丝螺母",null,"斤",1]
[53,"滑动变阻器","定做（大电阻大功率）","个",20]
[54,"STM32f103核心开发板","百科荣创STM32f103","套",2]
[55,"铺助触头","  施耐德   二开二闭","个",20]
[56,"数字型钳表","胜利vc606A","支",10]
[57,"精密螺丝刀",null,"套",2]
[58,"交流接触器","CJX2-2510/380V","只",30,null,null,"需到实验室现场更换或安装，并与实验室设备配"]
[59,"时间继电器","电子js14p  AC380V","个",10,null,null,"需到实验室现场更换或安装，并与实验室设备配"]
[60,"热继电器","JR36-20正泰或环宇电器","个",30,null,null,"需到实验室现场更换或安装，并与实验室设备配"]
[61,"小型通用 继电器","JTX-2C’AC36V","个",10,null,null,"需到实验室现场更换或安装，并与实验室设备配"]
[62,"辅助触头","F4-22正泰或环宇电器","个",30,null,null,"需到实验室现场更换或安装，并与实验室设备配"]
[63,"四极插头","25A  三相","个",10]
[64,"三位按钮","NP2-E3001 正泰或环宇电器","个",5]
[65,"触摸屏通讯线","4米","条",5]
[66,"网络线","4米","条",5]
[67,"风枪（焊枪）",null,"支",2]
[68,"接地电阻测量仪\n","需定做测试板","套",1]
[69,"塑料椅子",null,"只",30]
[70,"钉子机",null,"个",2]
[71,"两位开关面板","中兴","个",14]
[72,"两极自动开关带漏电","西门子2p带漏电","个",10]
[73,"单极自动开关","西门子1P","个",20]
[74,"U型双头插线","定做 双头4厘    50cm  多种颜色","袋",3]
["合计（元）："]